Mitsubishi Heavy Industries SRK / SRC 25 ZS-W

* **Designer model** – created to meet the demanding European taste for air conditioning systems. There are three different color options for a wider choice, depending on the style of the interior.
* **High seasonal efficiency** – A +++ / A ++
* **Extremely low noise levels** – up to 19 dB (A)
* **Ability to save favorite settings**
* **Quiet and even air flow** – through the “3D Auto” function to achieve a uniform temperature in all parts of the room.
* **Allergen-deactivating system** – activated with just one button.
* [**Wi-Fi adapter** (optional)](https://condex.bg/en/product-details/wi-fi-adapter-am-mhi-01/) – can be controlled by smartphones and tablets.
* **Improved control in “Auto” mode** – for cooling / heating switching.
* **LED indicator brightness** – can be adjusted.
* **Easy to use wireless infrared remote control** – for temperature control, ventilation speed, heating, cooling, drying modes. With many setting options, such as “Economy” for energy saving, weekly timer to be programmed according to individual needs, quiet mode “Silent”, which can be selected for the night, etc.

| **SRK / SRC 25 ZS-W** |  |
| --- | --- |
| Cooling capacity, kW: | 2.5 (0.9-3.1) |
| Heating capacity, kW: | 3.2 (0.9-4.5) |
| Cooling consumption, kW: | 0.62 |
| Heating consumption, kW: | 0.74 |
| EER/COP: | 4.03/4.32 |
| SEER/SCOP: | 8.50/4.70 |
| Energy class: | A+++/A++ |
| Cooling noise level, dB (A): | 19 / 23 / 28 / 36 |
| Heating noise level, dB (A): | 19 / 24 / 30 / 39 |
| Internal dimensions (h / d / w), mm: | 290 x 870 x 230 |
| External dimensions (h / d / w), mm: | 540 x 780(+62) x 290 |
| Refrigerant: | R32 |